(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "SX7H SHIFER MIAN SCH")
    (date "2022-07-18")
    (rev "V03")
    (company "宁波正朗汽车零部件有限公司")
    (comment 1 "批准:")
    (comment 2 "校准：")
    (comment 3 "设计：Ethan")
  )
  (lib_symbols
    (symbol "C_1" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_1" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_1_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_2" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_2" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_2_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_2_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_3" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_3" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_3_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_3_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_4" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_4" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_4_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_4_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Connector:TestPoint_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 3.81 0))
      (property "Value" "TestPoint_Small" (id 1) (at 0 2.032 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_Small_0_1"
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "TestPoint_Small_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:D_TVS_Dual_AAC" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 4.445 0))
      (property "Value" "D_TVS_Dual_AAC" (id 1) (at 0 2.54 0))
      (property "Footprint" "" (id 2) (at -3.81 0 0))
      (property "Datasheet" "~" (id 3) (at -3.81 0 0))
      (property "ki_keywords" "diode TVS thyrector" (id 4) (at 0 0 0))
      (property "ki_description" "Bidirectional dual transient-voltage-suppression diode, center on pin 3" (id 5) (at 0 0 0))
      (symbol "D_TVS_Dual_AAC_0_0"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 0)
          )
          (fill (type none))
        )
      )
      (symbol "D_TVS_Dual_AAC_0_1"
        (polyline
          (pts
            (xy -6.35 0)
            (xy 6.35 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.302 1.27)
            (xy -3.81 1.27)
            (xy -3.81 -1.27)
            (xy -4.318 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 1.27)
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.302 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 1.27)
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -6.35 -1.27)
            (xy -6.35 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.35 1.27)
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 6.35 -1.27)
            (xy 6.35 1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "D_TVS_Dual_AAC_1_1"
        (pin passive line (at -8.89 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 8.89 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "common")
          (number "3")
        )
      )
    )
    (symbol "Device:L_Coupled_1243" (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at 0 4.445 0))
      (property "Value" "L_Coupled_1243" (id 1) (at 0 -4.445 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic coupled" (id 4) (at 0 0 0))
      (property "ki_description" "Coupled inductor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_Coupled_1243_0_1"
        (circle (center -3.048 -1.27) (radius 0.254)
          (fill (type outline))
        )
        (circle (center -3.048 1.524) (radius 0.254)
          (fill (type outline))
        )
        (arc (start -2.54 2.032) (mid -2.032 1.524) (end -1.524 2.032)
          (fill (type none))
        )
        (arc (start -1.524 -2.032) (mid -2.032 -1.524) (end -2.54 -2.032)
          (fill (type none))
        )
        (arc (start -1.524 2.032) (mid -1.016 1.524) (end -0.508 2.032)
          (fill (type none))
        )
        (arc (start -0.508 -2.032) (mid -1.016 -1.524) (end -1.524 -2.032)
          (fill (type none))
        )
        (arc (start -0.508 2.032) (mid 0 1.524) (end 0.508 2.032)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.032)
            (xy -2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.032)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.032)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 2.032)
          )
          (fill (type none))
        )
        (arc (start 0.508 -2.032) (mid 0 -1.524) (end -0.508 -2.032)
          (fill (type none))
        )
        (arc (start 0.508 2.032) (mid 1.016 1.524) (end 1.524 2.032)
          (fill (type none))
        )
        (arc (start 1.524 -2.032) (mid 1.016 -1.524) (end 0.508 -2.032)
          (fill (type none))
        )
        (arc (start 1.524 2.032) (mid 2.032 1.524) (end 2.54 2.032)
          (fill (type none))
        )
        (arc (start 2.54 -2.032) (mid 2.032 -1.524) (end 1.524 -2.032)
          (fill (type none))
        )
      )
      (symbol "L_Coupled_1243_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "3")
          (number "3")
        )
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "4")
          (number "4")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer" "" (id 4) (at 0 0 0))
      (property "Description" "" (id 5) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 7) (at 0 0 0))
      (property "ki_description" "Resistor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 9) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Interface_CAN_LIN:TJA1042T" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -10.16 8.89 0))
      (property "Value" "TJA1042T" (id 1) (at 1.27 8.89 0))
      (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -12.7 0))
      (property "Datasheet" "http://www.nxp.com/documents/data_sheet/TJA1042.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "High-Speed CAN Transceiver" (id 4) (at 0 0 0))
      (property "ki_description" "High-Speed CAN Transceiver, standby mode, split pin, SOIC-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0))
      (symbol "TJA1042T_0_1"
        (rectangle (start -10.16 7.62) (end 10.16 -7.62)
          (fill (type background))
        )
      )
      (symbol "TJA1042T_1_1"
        (pin input line (at -12.7 5.08 0) (length 2.54)
          (name "TXD")
          (number "1")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_in line (at 0 10.16 270) (length 2.54)
          (name "VCC")
          (number "3")
        )
        (pin output line (at -12.7 2.54 0) (length 2.54)
          (name "RXD")
          (number "4")
        )
        (pin power_out line (at 12.7 0 180) (length 2.54)
          (name "SPLIT")
          (number "5")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "CANL")
          (number "6")
        )
        (pin bidirectional line (at 12.7 2.54 180) (length 2.54)
          (name "CANH")
          (number "7")
        )
        (pin input line (at -12.7 -5.08 0) (length 2.54)
          (name "STB")
          (number "8")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 148.59 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 148.59 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 164.7703 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 83.82) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 123.19 93.98) (xy 134.62 93.98)))
  (wire (pts (xy 134.62 86.36) (xy 135.89 86.36)))
  (wire (pts (xy 134.62 93.98) (xy 134.62 86.36)))
  (wire (pts (xy 82.55 83.82) (xy 88.9 83.82)))
  (wire (pts (xy 123.19 72.39) (xy 134.62 72.39)))
  (wire (pts (xy 134.62 72.39) (xy 134.62 81.28)))
  (wire (pts (xy 134.62 81.28) (xy 135.89 81.28)))
  (wire (pts (xy 107.95 86.36) (xy 110.49 86.36)))
  (wire (pts (xy 110.49 86.36) (xy 110.49 93.98)))
  (wire (pts (xy 123.19 80.01) (xy 123.19 83.82)))
  (wire (pts (xy 123.19 83.82) (xy 123.19 86.36)))
  (wire (pts (xy 88.9 83.82) (xy 91.44 83.82)))
  (wire (pts (xy 78.74 92.71) (xy 78.74 93.98)))
  (wire (pts (xy 93.98 86.36) (xy 93.98 93.98)))
  (wire (pts (xy 97.79 86.36) (xy 93.98 86.36)))
  (wire (pts (xy 161.29 78.74) (xy 165.1 78.74)))
  (wire (pts (xy 165.1 78.74) (xy 165.1 77.47)))
  (wire (pts (xy 161.29 88.9) (xy 165.1 88.9)))
  (wire (pts (xy 165.1 88.9) (xy 166.37 88.9)))
  (wire (pts (xy 102.87 72.39) (xy 110.49 72.39)))
  (wire (pts (xy 110.49 72.39) (xy 123.19 72.39)))
  (wire (pts (xy 73.66 93.98) (xy 78.74 93.98)))
  (wire (pts (xy 78.74 93.98) (xy 88.9 93.98)))
  (wire (pts (xy 173.99 86.36) (xy 177.8 86.36)))
  (wire (pts (xy 123.19 83.82) (xy 135.89 83.82)))
  (wire (pts (xy 88.9 72.39) (xy 93.98 72.39)))
  (wire (pts (xy 93.98 72.39) (xy 95.25 72.39)))
  (wire (pts (xy 140.97 93.98) (xy 148.59 93.98)))
  (wire (pts (xy 173.99 88.9) (xy 177.8 88.9)))
  (wire (pts (xy 88.9 93.98) (xy 93.98 93.98)))
  (wire (pts (xy 93.98 93.98) (xy 95.25 93.98)))
  (wire (pts (xy 148.59 93.98) (xy 148.59 96.52)))
  (wire (pts (xy 148.59 96.52) (xy 148.59 99.06)))
  (wire (pts (xy 78.74 72.39) (xy 78.74 74.93)))
  (wire (pts (xy 148.59 67.31) (xy 148.59 73.66)))
  (wire (pts (xy 165.1 67.31) (xy 165.1 69.85)))
  (wire (pts (xy 93.98 81.28) (xy 93.98 72.39)))
  (wire (pts (xy 97.79 81.28) (xy 93.98 81.28)))
  (wire (pts (xy 102.87 93.98) (xy 110.49 93.98)))
  (wire (pts (xy 110.49 93.98) (xy 123.19 93.98)))
  (wire (pts (xy 148.59 93.98) (xy 156.21 93.98)))
  (wire (pts (xy 107.95 81.28) (xy 110.49 81.28)))
  (wire (pts (xy 110.49 81.28) (xy 110.49 72.39)))
  (wire (pts (xy 88.9 80.01) (xy 88.9 83.82)))
  (wire (pts (xy 88.9 83.82) (xy 88.9 86.36)))
  (wire (pts (xy 161.29 86.36) (xy 164.7703 86.36)))
  (wire (pts (xy 164.7703 86.36) (xy 166.37 86.36)))
  (wire (pts (xy 73.66 72.39) (xy 78.74 72.39)))
  (wire (pts (xy 78.74 72.39) (xy 88.9 72.39)))
  (wire (pts (xy 165.1 78.74) (xy 177.8 78.74)))
  (hierarchical_label "CANH" (shape input) (at 73.66 93.98 180))
  (hierarchical_label "CAN_RX" (shape input) (at 177.8 86.36 0))
  (hierarchical_label "CAN_STB" (shape input) (at 177.8 78.74 0))
  (hierarchical_label "CAN_TX" (shape input) (at 177.8 88.9 0))
  (hierarchical_label "CANL" (shape input) (at 73.66 72.39 180))
  (symbol (lib_id "power:GND") (at 148.59 67.31 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0179" (id 0) (at 148.59 60.96 0))
    (property "Value" "GND" (id 1) (at 150.495 66.519 0))
    (property "Footprint" "" (id 2) (at 148.59 67.31 0))
    (property "Datasheet" "" (id 3) (at 148.59 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 115.57 83.82 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0177" (id 0) (at 109.22 83.82 0))
    (property "Value" "GND" (id 1) (at 111.1251 81.759 0))
    (property "Footprint" "" (id 2) (at 115.57 83.82 0))
    (property "Datasheet" "" (id 3) (at 115.57 83.82 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 165.1 73.66 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R152" (id 0) (at 163.9275 69.85 90))
    (property "Value" "10k" (id 1) (at 165.4326 74.93 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 166.878 73.66 90))
    (property "Datasheet" "~" (id 3) (at 165.1 73.66 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 165.1 73.66 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 165.1 73.66 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 165.1 73.66 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 165.1 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 170.18 88.9 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R154" (id 0) (at 175.26 87.7275 90))
    (property "Value" "0R" (id 1) (at 170.18 89.2326 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 170.18 90.678 90))
    (property "Datasheet" "~" (id 3) (at 170.18 88.9 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 170.18 88.9 0))
    (property "Description" "RES 0R 1% 1/10W 0603" (id 5) (at 170.18 88.9 0))
    (property "Manufacturer Product Number" "AECR0603F0000K9" (id 6) (at 170.18 88.9 0))
    (property "Descriptions" "RES 0R 1% 1/10W 0603" (id 7) (at 170.18 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 91.44 83.82 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0176" (id 0) (at 97.79 83.82 0))
    (property "Value" "GND" (id 1) (at 95.8849 85.881 0))
    (property "Footprint" "" (id 2) (at 91.44 83.82 0))
    (property "Datasheet" "" (id 3) (at 91.44 83.82 0))
    (pin "1")
  )
  (symbol (lib_id "Device:L_Coupled_1243") (at 102.87 83.82 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L104" (id 0) (at 102.87 77.0594 0))
    (property "Value" "DLW43SH510XK" (id 1) (at 102.87 79.8345 0))
    (property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_1812CAN" (id 2) (at 102.87 83.82 0))
    (property "Datasheet" "~" (id 3) (at 102.87 83.82 0))
    (property "Description" "CMC 51UH 230MA 2LN SMD AEC-Q200" (id 4) (at 102.87 83.82 0))
    (property "Manufacturer" "Murata Electronics" (id 5) (at 102.87 83.82 0))
    (property "Manufacturer Product Number" "DLW43SH510XK2L" (id 6) (at 102.87 83.82 0))
    (property "Descriptions" "CMC 51UH 230MA 2LN SMD AEC-Q200" (id 7) (at 102.87 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 123.19 83.82 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP93" (id 0) (at 123.063 81.759 0))
    (property "Value" "TestPoint_Small" (id 1) (at 123.19 85.852 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 118.11 83.82 0))
    (property "Datasheet" "~" (id 3) (at 118.11 83.82 0))
    (pin "1")
  )
  (symbol (lib_name "C_4") (lib_id "Device:C") (at 156.21 97.79 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C148" (id 0) (at 151.511 95.6115 0))
    (property "Value" "10uF/6.3V" (id 1) (at 161.671 103.4666 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 157.1752 101.6 0))
    (property "Datasheet" "~" (id 3) (at 156.21 97.79 0))
    (property "Manufacturer Product Number" "CC0805KKX7R5BB106" (id 4) (at 156.21 97.79 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 156.21 97.79 0))
    (property "Description" "CAP CER 10UF 6.3V X7R 0805" (id 6) (at 156.21 97.79 0))
    (property "Descriptions" "CAP CER 10UF 6.3V X7R 0805" (id 7) (at 156.21 97.79 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 123.19 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R151" (id 0) (at 124.968 89.2615 0))
    (property "Value" "10k" (id 1) (at 124.968 92.0366 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 121.412 90.17 90))
    (property "Datasheet" "~" (id 3) (at 123.19 90.17 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 123.19 90.17 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 123.19 90.17 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 123.19 90.17 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 123.19 90.17 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 140.97 97.79 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C147" (id 0) (at 142.621 95.6115 0))
    (property "Value" "100nF/50V" (id 1) (at 136.271 103.4666 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 141.9352 101.6 0))
    (property "Datasheet" "~" (id 3) (at 140.97 97.79 0))
    (property "Manufacturer Product Number" " AC0603KRX7R9BB104" (id 4) (at 140.97 97.79 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 140.97 97.79 0))
    (property "Description" "CAP CER 100nF 50V X7R 0603" (id 6) (at 140.97 97.79 0))
    (property "Descriptions" "CAP CER 100nF 50V X7R 0603" (id 7) (at 140.97 97.79 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 170.18 86.36 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R153" (id 0) (at 175.26 85.1875 90))
    (property "Value" "0R" (id 1) (at 168.91 86.6926 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 170.18 88.138 90))
    (property "Datasheet" "~" (id 3) (at 170.18 86.36 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 170.18 86.36 0))
    (property "Description" "RES 0R 1% 1/10W 0603" (id 5) (at 170.18 86.36 0))
    (property "Manufacturer Product Number" "AECR0603F0000K9" (id 6) (at 170.18 86.36 0))
    (property "Descriptions" "RES 0R 1% 1/10W 0603" (id 7) (at 170.18 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_3") (lib_id "Device:C") (at 119.38 83.82 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C146" (id 0) (at 118.4715 78.359 0))
    (property "Value" "4.7nF/50V" (id 1) (at 122.5166 80.899 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 123.19 82.8548 0))
    (property "Datasheet" "~" (id 3) (at 119.38 83.82 0))
    (property "Manufacturer Product Number" "AC0603KRX7R9BB472" (id 4) (at 119.38 83.82 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 119.38 83.82 0))
    (property "Description" "CAP CER 4700PF 50V X7R 0603" (id 6) (at 119.38 83.82 0))
    (property "Descriptions" "CAP CER 4700PF 50V X7R 0603" (id 7) (at 119.38 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 99.06 72.39 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R148" (id 0) (at 99.06 67.4075 90))
    (property "Value" "0R" (id 1) (at 99.06 70.1826 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 99.06 74.168 90))
    (property "Datasheet" "~" (id 3) (at 99.06 72.39 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 99.06 72.39 0))
    (property "Description" "RES 0R 1% 1/10W 0603" (id 5) (at 99.06 72.39 0))
    (property "Manufacturer Product Number" "AECR0603F0000K9" (id 6) (at 99.06 72.39 0))
    (property "Descriptions" "RES 0R 1% 1/10W 0603" (id 7) (at 99.06 72.39 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 148.59 96.52 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP94" (id 0) (at 149.733 96.999 0))
    (property "Value" "TestPoint_Small" (id 1) (at 148.59 98.552 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 143.51 96.52 0))
    (property "Datasheet" "~" (id 3) (at 143.51 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 123.19 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R150" (id 0) (at 124.968 75.2915 0))
    (property "Value" "10k" (id 1) (at 124.968 78.0666 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 121.412 76.2 90))
    (property "Datasheet" "~" (id 3) (at 123.19 76.2 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 123.19 76.2 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 123.19 76.2 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 123.19 76.2 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 123.19 76.2 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 110.49 93.98 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP92" (id 0) (at 109.093 95.729 0))
    (property "Value" "TestPoint_Small" (id 1) (at 110.49 96.012 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 105.41 93.98 0))
    (property "Datasheet" "~" (id 3) (at 105.41 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 164.7703 86.36 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP95" (id 0) (at 162.1033 84.299 0))
    (property "Value" "TestPoint_Small" (id 1) (at 164.7703 88.392 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 159.6903 86.36 0))
    (property "Datasheet" "~" (id 3) (at 159.6903 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 148.59 99.06 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0180" (id 0) (at 148.59 95.25 0))
    (property "Value" "+5V" (id 1) (at 149.987 100.8089 0))
    (property "Footprint" "" (id 2) (at 148.59 99.06 0))
    (property "Datasheet" "" (id 3) (at 148.59 99.06 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 99.06 93.98 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R149" (id 0) (at 99.06 88.9975 90))
    (property "Value" "0R" (id 1) (at 99.06 91.7726 90))
    (property "Footprint" "GODPP:R0603" (id 2) (at 99.06 95.758 90))
    (property "Datasheet" "~" (id 3) (at 99.06 93.98 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 99.06 93.98 0))
    (property "Description" "RES 0R 1% 1/10W 0603" (id 5) (at 99.06 93.98 0))
    (property "Manufacturer Product Number" "AECR0603F0000K9" (id 6) (at 99.06 93.98 0))
    (property "Descriptions" "RES 0R 1% 1/10W 0603" (id 7) (at 99.06 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Interface_CAN_LIN:TJA1042T") (at 148.59 83.82 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U104" (id 0) (at 148.59 69.8204 0))
    (property "Value" "TJA1042T" (id 1) (at 148.59 72.5955 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 148.59 71.12 0))
    (property "Datasheet" "http://www.nxp.com/documents/data_sheet/TJA1042.pdf" (id 3) (at 148.59 83.82 0))
    (property "Description" "IC TRANSCEIVER HALF 1/1 8SO" (id 4) (at 148.59 83.82 0))
    (property "Manufacturer" "NXP USA Inc." (id 5) (at 148.59 83.82 0))
    (property "Manufacturer Product Number" "TJA1042T" (id 6) (at 148.59 83.82 0))
    (property "Descriptions" "IC TRANSCEIVER HALF 1/1 8SO" (id 7) (at 148.59 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 140.97 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0178" (id 0) (at 140.97 107.95 0))
    (property "Value" "GND" (id 1) (at 138.909 106.0449 0))
    (property "Footprint" "" (id 2) (at 140.97 101.6 0))
    (property "Datasheet" "" (id 3) (at 140.97 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 165.1 88.9 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP96" (id 0) (at 162.433 90.649 0))
    (property "Value" "TestPoint_Small" (id 1) (at 165.1 90.932 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 160.02 88.9 0))
    (property "Datasheet" "~" (id 3) (at 160.02 88.9 0))
    (pin "1")
  )
  (symbol (lib_name "C_2") (lib_id "Device:C") (at 88.9 90.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C145" (id 0) (at 90.551 87.9915 0))
    (property "Value" "100pF/50V" (id 1) (at 84.201 95.8466 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 89.8652 93.98 0))
    (property "Datasheet" "~" (id 3) (at 88.9 90.17 0))
    (property "Description" "CAP CER 100PF 50V C0G 0603" (id 4) (at 88.9 90.17 0))
    (property "Manufacturer Product Number" "AC0603JRNPO9BN101" (id 5) (at 88.9 90.17 0))
    (property "Manufacturer" "YAGEO" (id 6) (at 88.9 90.17 0))
    (property "Descriptions" "CAP CER 100PF 50V C0G 0603" (id 7) (at 88.9 90.17 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 165.1 67.31 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0182" (id 0) (at 165.1 60.96 0))
    (property "Value" "GND" (id 1) (at 167.005 66.519 0))
    (property "Footprint" "" (id 2) (at 165.1 67.31 0))
    (property "Datasheet" "" (id 3) (at 165.1 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 156.21 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0181" (id 0) (at 156.21 107.95 0))
    (property "Value" "GND" (id 1) (at 154.149 106.0449 0))
    (property "Footprint" "" (id 2) (at 156.21 101.6 0))
    (property "Datasheet" "" (id 3) (at 156.21 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_TVS_Dual_AAC") (at 78.74 83.82 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D108" (id 0) (at 76.708 82.9115 90))
    (property "Value" "NUP2105LT1G" (id 1) (at 76.708 85.6866 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 78.74 80.01 0))
    (property "Datasheet" "~" (id 3) (at 78.74 80.01 0))
    (property "Manufacturer Product Number" "NUP2105LT1G" (id 4) (at 78.74 83.82 90))
    (property "Manufacturer" "onsemi" (id 5) (at 78.74 83.82 90))
    (property "Description" "TVS DIODE 24VWM 44VC SOT23-3" (id 6) (at 78.74 83.82 90))
    (property "Descriptions" "TVS DIODE 24VWM 44VC SOT23-3" (id 7) (at 78.74 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 110.49 72.39 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP91" (id 0) (at 109.093 70.329 0))
    (property "Value" "TestPoint_Small" (id 1) (at 110.49 74.422 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 105.41 72.39 0))
    (property "Datasheet" "~" (id 3) (at 105.41 72.39 0))
    (pin "1")
  )
  (symbol (lib_name "C_1") (lib_id "Device:C") (at 88.9 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C144" (id 0) (at 90.551 74.0215 0))
    (property "Value" "100pF/50V" (id 1) (at 84.201 81.8766 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 89.8652 80.01 0))
    (property "Datasheet" "~" (id 3) (at 88.9 76.2 0))
    (property "Description" "CAP CER 100PF 50V C0G 0603" (id 4) (at 88.9 76.2 0))
    (property "Manufacturer Product Number" "AC0603JRNPO9BN101" (id 5) (at 88.9 76.2 0))
    (property "Manufacturer" "YAGEO" (id 6) (at 88.9 76.2 0))
    (property "Descriptions" "CAP CER 100PF 50V C0G 0603" (id 7) (at 88.9 76.2 0))
    (pin "1")
    (pin "2")
  )
)
