(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "SX7H SHIFER MIAN SCH")
    (date "2022-07-18")
    (rev "V03")
    (company "宁波正朗汽车零部件有限公司")
    (comment 1 "批准:")
    (comment 2 "校准：")
    (comment 3 "设计：Ethan")
  )
  (lib_symbols
    (symbol "C_1" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_1" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_1_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_2" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_2" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_2_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_2_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_4" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_4" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_4_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_4_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_7" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_7" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_7_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_7_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_8" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_8" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_8_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_8_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "C_9" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_9" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_9_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_9_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Connector:TestPoint_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 3.81 0))
      (property "Value" "TestPoint_Small" (id 1) (at 0 2.032 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_Small_0_1"
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "TestPoint_Small_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Device:C_Polarized_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Polarized_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_Small_0_1"
        (rectangle (start -1.524 -0.3048) (end 1.524 -0.6858)
          (fill (type outline))
        )
        (rectangle (start -1.524 0.6858) (end 1.524 0.3048)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.524)
            (xy -0.762 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.27)
            (xy -1.016 1.778)
          )
          (fill (type none))
        )
      )
      (symbol "C_Polarized_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.8542)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.8542)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:D" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "Diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:D_Schottky_Filled" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D_Schottky_Filled" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "Schottky diode, filled shape" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_Schottky_Filled_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "D_Schottky_Filled_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:D_TVS" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D_TVS" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode TVS thyrector" (id 4) (at 0 0 0))
      (property "ki_description" "Bidirectional transient-voltage-suppression diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_TVS_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy -0.508 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
            (xy 2.54 1.27)
            (xy 2.54 -1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_TVS_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Ferrite" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "L_Ferrite" (id 1) (at 2.794 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor with ferrite core" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_Ferrite_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -2.794)
            (xy 1.016 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.778)
            (xy 1.016 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -0.762)
            (xy 1.016 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0.254)
            (xy 1.016 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 1.016 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 2.286)
            (xy 1.016 2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -2.286)
            (xy 1.524 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -1.27)
            (xy 1.524 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -0.254)
            (xy 1.524 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 0.762)
            (xy 1.524 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 1.778)
            (xy 1.524 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 2.794)
            (xy 1.524 2.286)
          )
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_Ferrite_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:Q_NPN_BEC_BRT" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 3.81 1.27 0))
      (property "Value" "Q_NPN_BEC_BRT" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0))
      (property "ki_description" "NPN bias resistor transistor, base/emitter/collector" (id 5) (at 0 0 0))
      (symbol "Q_NPN_BEC_BRT_0_1"
        (rectangle (start -6.35 0.508) (end -4.826 -0.508)
          (fill (type none))
        )
        (rectangle (start -4.318 -2.286) (end -3.302 -0.762)
          (fill (type none))
        )
        (circle (center -3.81 0) (radius 0.254)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -3.81 -0.762)
            (xy -3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 0)
            (xy -4.826 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 1.524)
            (xy -0.635 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -2.286)
            (xy -3.81 -3.048)
            (xy 1.27 -3.048)
          )
          (fill (type none))
        )
        (circle (center 1.27 -3.048) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "Q_NPN_BEC_BRT_1_1"
        (polyline
          (pts
            (xy -0.635 0.635)
            (xy 1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -0.635)
            (xy 1.27 -2.54)
            (xy 1.27 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.778)
            (xy 0.508 -1.27)
            (xy 1.016 -2.286)
            (xy 0 -1.778)
            (xy 0 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 0 0) (radius 2.8194)
          (fill (type none))
        )
        (pin input line (at -8.89 0 0) (length 2.54)
          (name "B")
          (number "1")
        )
        (pin passive line (at 1.27 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 1.27 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer" "" (id 4) (at 0 0 0))
      (property "Description" "" (id 5) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 7) (at 0 0 0))
      (property "ki_description" "Resistor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 9) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:BAV70" (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0.635 -2.54 0))
      (property "Value" "BAV70" (id 1) (at 0 2.54 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "Dual 100V 215mA high-speed switching diodes, common cathode, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "BAV70_0_1"
        (polyline
          (pts
            (xy -3.81 0)
            (xy 3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -1.27 0)
            (xy -3.81 -1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -1.27)
            (xy 1.27 0)
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.81 -1.27)
            (xy 3.81 -1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
        (pin passive line (at -7.62 0 0) (length 3.81)
          (name "A")
          (number "1")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "A")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "K")
          (number "3")
        )
      )
    )
    (symbol "Diode:BAV99S" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "BAV99S" (id 1) (at 0 5.08 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 0 -12.7 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "Diode" (id 5) (at 0 0 0))
      (property "ki_description" "High-speed switching diodes, dual series, SOT-363" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOT?363*" (id 7) (at 0 0 0))
      (symbol "BAV99S_0_1"
        (polyline
          (pts
            (xy -5.08 0)
            (xy 5.08 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.81 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -1.27 0)
            (xy -3.81 -1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 3.81 0)
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 1.27 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "BAV99S_1_1"
        (polyline
          (pts
            (xy 6.35 0)
            (xy 7.62 0)
          )
          (fill (type none))
        )
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "K2")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "K3A4")
          (number "6")
        )
      )
      (symbol "BAV99S_2_1"
        (polyline
          (pts
            (xy 6.35 0)
            (xy 7.62 0)
          )
          (fill (type none))
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "K1A2")
          (number "3")
        )
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "A3")
          (number "4")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "K4")
          (number "5")
        )
      )
    )
    (symbol "Regulator_Linear:MCP1703A-1202_SOT223" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "MCP1703A-1202_SOT223" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (id 2) (at 0 5.08 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf" (id 3) (at 0 -1.27 0))
      (property "ki_keywords" "REGULATOR LDO" (id 4) (at 0 0 0))
      (property "ki_description" "Low Quiescent Current LDO Regulator, 1.2V, 250mA, Vin<=16V, SOT-223" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?223*TabPin2*" (id 6) (at 0 0 0))
      (symbol "MCP1703A-1202_SOT223_0_1"
        (rectangle (start -5.08 -5.08) (end 5.08 1.905)
          (fill (type background))
        )
      )
      (symbol "MCP1703A-1202_SOT223_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "3")
        )
      )
    )
    (symbol "Transistor_BJT:BCP53" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "BCP53" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BCP53T1-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "PNP Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "1A Ic, 80V Vce, PNP Medium Power Transistor, SOT-223" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?223*" (id 6) (at 0 0 0))
      (symbol "BCP53_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.778)
            (xy 1.778 -2.286)
            (xy 1.27 -1.27)
            (xy 2.286 -1.778)
            (xy 2.286 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BCP53_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "3")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54) hide
          (name "C")
          (number "4")
        )
      )
    )
    (symbol "power:+12P" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+12P" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+12P\"" (id 5) (at 0 0 0))
      (symbol "+12P_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+12P_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+12P")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 39.37 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 95.25 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 130.81 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 193.04 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 166.37 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 38.1 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 110.49) (diameter 0) (color 0 0 0 0))
  (junction (at 115.57 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 180.34 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 166.37) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 148.59) (diameter 0) (color 0 0 0 0))
  (junction (at 219.71 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 48.26 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 189.23 116.84) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 62.23 133.35) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 35.56 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 119.38) (diameter 0) (color 0 0 0 0))
  (junction (at 38.1 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 110.49) (diameter 0) (color 0 0 0 0))
  (junction (at 48.26 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 200.66 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 180.34 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 200.66 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 189.23 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 217.17 29.21) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 189.23 116.84) (xy 196.85 116.84)))
  (wire (pts (xy 196.85 116.84) (xy 196.85 113.03)))
  (wire (pts (xy 217.17 29.21) (xy 219.71 29.21)))
  (wire (pts (xy 219.71 29.21) (xy 226.06 29.21)))
  (wire (pts (xy 137.16 148.59) (xy 144.78 148.59)))
  (wire (pts (xy 71.12 102.87) (xy 78.74 102.87)))
  (wire (pts (xy 152.4 113.03) (xy 152.4 116.84)))
  (wire (pts (xy 152.4 116.84) (xy 166.37 116.84)))
  (wire (pts (xy 144.78 102.87) (xy 144.78 128.27)))
  (wire (pts (xy 182.88 43.18) (xy 182.88 45.72)))
  (wire (pts (xy 182.88 45.72) (xy 200.66 45.72)))
  (wire (pts (xy 200.66 29.21) (xy 200.66 33.02)))
  (wire (pts (xy 33.02 125.73) (xy 35.56 125.73)))
  (wire (pts (xy 35.56 125.73) (xy 38.1 125.73)))
  (wire (pts (xy 162.56 139.7) (xy 162.56 143.51)))
  (wire (pts (xy 137.16 102.87) (xy 137.16 105.41)))
  (wire (pts (xy 29.21 140.97) (xy 31.75 140.97)))
  (wire (pts (xy 137.16 113.03) (xy 137.16 118.11)))
  (wire (pts (xy 182.88 45.72) (xy 182.88 48.26)))
  (wire (pts (xy 173.99 102.87) (xy 180.34 102.87)))
  (wire (pts (xy 180.34 102.87) (xy 189.23 102.87)))
  (wire (pts (xy 189.23 102.87) (xy 189.23 105.41)))
  (wire (pts (xy 83.82 110.49) (xy 83.82 111.76)))
  (wire (pts (xy 180.34 102.87) (xy 180.34 105.41)))
  (wire (pts (xy 68.58 157.48) (xy 68.58 161.29)))
  (wire (pts (xy 177.8 29.21) (xy 182.88 29.21)))
  (wire (pts (xy 182.88 29.21) (xy 193.04 29.21)))
  (wire (pts (xy 162.56 139.7) (xy 165.1 139.7)))
  (wire (pts (xy 217.17 29.21) (xy 217.17 33.02)))
  (wire (pts (xy 88.9 102.87) (xy 95.25 102.87)))
  (wire (pts (xy 95.25 102.87) (xy 106.68 102.87)))
  (wire (pts (xy 106.68 102.87) (xy 115.57 102.87)))
  (wire (pts (xy 95.25 114.3) (xy 95.25 116.84)))
  (wire (pts (xy 137.16 147.32) (xy 137.16 148.59)))
  (wire (pts (xy 166.37 110.49) (xy 166.37 116.84)))
  (wire (pts (xy 166.37 116.84) (xy 166.37 118.11)))
  (wire (pts (xy 200.66 45.72) (xy 217.17 45.72)))
  (wire (pts (xy 115.57 102.87) (xy 115.57 107.95)))
  (wire (pts (xy 31.75 102.87) (xy 38.1 102.87)))
  (wire (pts (xy 38.1 102.87) (xy 38.1 106.68)))
  (wire (pts (xy 182.88 29.21) (xy 182.88 35.56)))
  (wire (pts (xy 52.07 153.67) (xy 52.07 157.48)))
  (wire (pts (xy 52.07 157.48) (xy 52.07 158.75)))
  (wire (pts (xy 46.99 140.97) (xy 52.07 140.97)))
  (wire (pts (xy 44.45 157.48) (xy 52.07 157.48)))
  (wire (pts (xy 71.12 110.49) (xy 78.74 110.49)))
  (wire (pts (xy 78.74 110.49) (xy 83.82 110.49)))
  (wire (pts (xy 95.25 102.87) (xy 95.25 106.68)))
  (wire (pts (xy 200.66 29.21) (xy 217.17 29.21)))
  (wire (pts (xy 137.16 139.7) (xy 144.78 139.7)))
  (wire (pts (xy 57.15 133.35) (xy 62.23 133.35)))
  (wire (pts (xy 62.23 133.35) (xy 73.66 133.35)))
  (wire (pts (xy 166.37 116.84) (xy 180.34 116.84)))
  (wire (pts (xy 180.34 116.84) (xy 189.23 116.84)))
  (wire (pts (xy 189.23 116.84) (xy 189.23 113.03)))
  (wire (pts (xy 52.07 157.48) (xy 58.42 157.48)))
  (wire (pts (xy 144.78 139.7) (xy 144.78 140.97)))
  (wire (pts (xy 115.57 113.03) (xy 115.57 116.84)))
  (wire (pts (xy 38.1 102.87) (xy 48.26 102.87)))
  (wire (pts (xy 48.26 102.87) (xy 48.26 106.68)))
  (wire (pts (xy 66.04 157.48) (xy 68.58 157.48)))
  (wire (pts (xy 68.58 157.48) (xy 72.39 157.48)))
  (wire (pts (xy 144.78 139.7) (xy 151.13 139.7)))
  (wire (pts (xy 217.17 40.64) (xy 217.17 45.72)))
  (wire (pts (xy 52.07 140.97) (xy 52.07 144.78)))
  (wire (pts (xy 52.07 144.78) (xy 52.07 146.05)))
  (wire (pts (xy 45.72 125.73) (xy 48.26 125.73)))
  (wire (pts (xy 48.26 125.73) (xy 52.07 125.73)))
  (wire (pts (xy 144.78 135.89) (xy 144.78 139.7)))
  (wire (pts (xy 115.57 102.87) (xy 130.81 102.87)))
  (wire (pts (xy 137.16 102.87) (xy 144.78 102.87)))
  (wire (pts (xy 144.78 102.87) (xy 152.4 102.87)))
  (wire (pts (xy 152.4 102.87) (xy 158.75 102.87)))
  (wire (pts (xy 180.34 113.03) (xy 180.34 116.84)))
  (wire (pts (xy 130.81 102.87) (xy 137.16 102.87)))
  (wire (pts (xy 200.66 40.64) (xy 200.66 45.72)))
  (wire (pts (xy 83.82 119.38) (xy 83.82 120.65)))
  (wire (pts (xy 189.23 102.87) (xy 196.85 102.87)))
  (wire (pts (xy 196.85 102.87) (xy 196.85 105.41)))
  (wire (pts (xy 158.75 139.7) (xy 162.56 139.7)))
  (wire (pts (xy 48.26 102.87) (xy 71.12 102.87)))
  (wire (pts (xy 44.45 165.1) (xy 44.45 166.37)))
  (wire (pts (xy 44.45 166.37) (xy 52.07 166.37)))
  (wire (pts (xy 152.4 102.87) (xy 152.4 105.41)))
  (wire (pts (xy 38.1 114.3) (xy 48.26 114.3)))
  (hierarchical_label "VCC12_C" (shape input) (at 33.02 125.73 180))
  (hierarchical_label "ILL" (shape input) (at 177.8 29.21 180))
  (hierarchical_label "KL30" (shape input) (at 31.75 102.87 180))
  (hierarchical_label "KL15" (shape input) (at 29.21 140.97 180))
  (hierarchical_label "WAKEUP_M" (shape input) (at 72.39 157.48 0))
  (hierarchical_label "POWER_M" (shape input) (at 165.1 139.7 0))
  (hierarchical_label "ILL_O" (shape input) (at 226.06 29.21 0))
  (symbol (lib_id "power:GND") (at 83.82 138.43 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0106" (id 0) (at 83.82 144.78 0))
    (property "Value" "GND" (id 1) (at 83.82 142.9924 0))
    (property "Footprint" "" (id 2) (at 83.82 138.43 0))
    (property "Datasheet" "" (id 3) (at 83.82 138.43 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 154.94 148.59 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 154.94 144.78 0))
    (property "Value" "+5V" (id 1) (at 152.4 152.4 0))
    (property "Footprint" "" (id 2) (at 154.94 148.59 0))
    (property "Datasheet" "" (id 3) (at 154.94 148.59 0))
    (pin "1")
  )
  (symbol (lib_name "C_7") (lib_id "Device:C") (at 189.23 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C110" (id 0) (at 190.881 107.0415 0))
    (property "Value" "100nF/50V" (id 1) (at 184.531 112.3566 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 190.1952 113.03 0))
    (property "Datasheet" "~" (id 3) (at 189.23 109.22 0))
    (property "Manufacturer Product Number" " AC0603KRX7R9BB104" (id 4) (at 189.23 109.22 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 189.23 109.22 0))
    (property "Description" "CAP CER 100nF 50V X7R 0603" (id 6) (at 189.23 109.22 0))
    (property "Descriptions" "CAP CER 100nF 50V X7R 0603" (id 7) (at 189.23 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 106.68 102.87 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP12" (id 0) (at 105.283 100.809 0))
    (property "Value" "TestPoint_Small" (id 1) (at 106.68 104.902 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 101.6 102.87 0))
    (property "Datasheet" "~" (id 3) (at 101.6 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12P") (at 130.81 95.25 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0109" (id 0) (at 130.81 99.06 0))
    (property "Value" "+12P" (id 1) (at 128.397 91.919 0))
    (property "Footprint" "" (id 2) (at 130.81 95.25 0))
    (property "Datasheet" "" (id 3) (at 130.81 95.25 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 95.25 116.84 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0107" (id 0) (at 95.25 123.19 0))
    (property "Value" "GND" (id 1) (at 95.25 121.4024 0))
    (property "Footprint" "" (id 2) (at 95.25 116.84 0))
    (property "Datasheet" "" (id 3) (at 95.25 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:BAV70") (at 52.07 133.35 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D103" (id 0) (at 50.038 132.4415 90))
    (property "Value" "BAV70" (id 1) (at 50.038 135.2166 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 52.07 133.35 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf" (id 3) (at 52.07 133.35 0))
    (property "Manufacturer Product Number" "BAV70LT1G" (id 4) (at 52.07 133.35 90))
    (property "Manufacturer" "onsemi" (id 5) (at 52.07 133.35 90))
    (property "Description" "DIODE ARRAY GP 100V 200MA SOT23" (id 6) (at 52.07 133.35 90))
    (property "Descriptions" "DIODE ARRAY GP 100V 200MA SOT23" (id 7) (at 52.07 133.35 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:GND") (at 52.07 166.37 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0105" (id 0) (at 52.07 172.72 0))
    (property "Value" "GND" (id 1) (at 52.07 170.9324 0))
    (property "Footprint" "" (id 2) (at 52.07 166.37 0))
    (property "Datasheet" "" (id 3) (at 52.07 166.37 0))
    (pin "1")
  )
  (symbol (lib_name "C_4") (lib_id "Device:C") (at 182.88 39.37 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C109" (id 0) (at 176.911 37.1915 0))
    (property "Value" "100nF/100V" (id 1) (at 169.291 42.5066 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 183.8452 43.18 0))
    (property "Datasheet" "~" (id 3) (at 182.88 39.37 0))
    (property "Manufacturer Product Number" "AC0805KKX7R0BB104" (id 4) (at 182.88 39.37 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 182.88 39.37 0))
    (property "Description" "CAP CER 0.1uF 100V X7R 0805" (id 6) (at 182.88 39.37 0))
    (property "Descriptions" "CAP CER 0.1uF 100V X7R 0805" (id 7) (at 182.88 39.37 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D") (at 196.85 29.21 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D105" (id 0) (at 196.85 23.9735 0))
    (property "Value" "S1G" (id 1) (at 196.85 26.7486 0))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 196.85 29.21 0))
    (property "Datasheet" "~" (id 3) (at 196.85 29.21 0))
    (property "Manufacturer Product Number" "S1G-13-F" (id 4) (at 196.85 29.21 0))
    (property "Manufacturer" "Diodes Incorporated" (id 5) (at 196.85 29.21 0))
    (property "Description" "DIODE GEN PURP 400V 1A SMA" (id 6) (at 196.85 29.21 0))
    (property "Descriptions" "DIODE GEN PURP 400V 1A SMA" (id 7) (at 196.85 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 39.37 140.97 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP3" (id 0) (at 37.973 143.989 0))
    (property "Value" "TestPoint_Small" (id 1) (at 39.37 143.002 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 34.29 140.97 0))
    (property "Datasheet" "~" (id 3) (at 34.29 140.97 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:BAV99S") (at 162.56 148.59 180) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D2" (id 0) (at 161.29 152.4 0))
    (property "Value" "BAV99S,115" (id 1) (at 161.29 154.94 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 162.56 135.89 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf" (id 3) (at 162.56 148.59 0))
    (property "Descriptions" "DIODE ARRAY GP 100V 200MA 6TSSOP" (id 4) (at 162.56 148.59 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 144.78 139.7 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP13" (id 0) (at 139.573 137.639 0))
    (property "Value" "TestPoint_Small" (id 1) (at 144.78 141.732 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 139.7 139.7 0))
    (property "Datasheet" "~" (id 3) (at 139.7 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Device:L_Ferrite") (at 154.94 139.7 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L102" (id 0) (at 154.94 134.3364 90))
    (property "Value" "1k@100MHz" (id 1) (at 154.94 137.1115 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 154.94 139.7 0))
    (property "Datasheet" "~" (id 3) (at 154.94 139.7 0))
    (property "Manufacturer Product Number" "BLM18RK102SN1D" (id 4) (at 154.94 139.7 90))
    (property "Manufacturer" "Murata Electronics" (id 5) (at 154.94 139.7 90))
    (property "Description" "FERRITEBEAD SMD AUTOMOTIVE POWER" (id 6) (at 154.94 139.7 90))
    (property "Descriptions" "FERRITEBEAD SMD AUTOMOTIVE POWER" (id 7) (at 154.94 139.7 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 130.81 99.06 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D4" (id 0) (at 128.27 100.0126 90))
    (property "Value" "BAS316" (id 1) (at 129.54 96.52 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 130.81 99.06 0))
    (property "Datasheet" "~" (id 3) (at 130.81 99.06 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 130.81 99.06 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 130.81 99.06 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 130.81 99.06 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized_Small") (at 115.57 110.49 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C104" (id 0) (at 117.729 109.5815 0))
    (property "Value" "47uF/35V" (id 1) (at 117.729 112.3566 0))
    (property "Footprint" "Capacitor_SMD:CP_Elec_6.3x9.9" (id 2) (at 115.57 110.49 0))
    (property "Datasheet" "~" (id 3) (at 115.57 110.49 0))
    (property "Manufacturer Product Number" "35THV47M6.3X8" (id 4) (at 115.57 110.49 0))
    (property "Manufacturer" "rubycon(红宝石)" (id 5) (at 115.57 110.49 0))
    (property "Description" "CAP ALUM 47UF 20% 35V SMD" (id 6) (at 115.57 110.49 0))
    (property "Descriptions" "CAP ALUM 47UF 20% 35V SMD" (id 7) (at 115.57 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D_TVS") (at 200.66 36.83 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D104" (id 0) (at 202.692 35.9215 90))
    (property "Value" "SMAJ33CA-AT" (id 1) (at 202.692 38.6966 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 200.66 36.83 0))
    (property "Datasheet" "~" (id 3) (at 200.66 36.83 0))
    (property "Manufacturer Product Number" "SMAJ33CA-AT" (id 4) (at 200.66 36.83 90))
    (property "Manufacturer" "" (id 5) (at 200.66 36.83 90))
    (property "Description" "TVS 35.7V 7.5A SMA" (id 6) (at 200.66 36.83 0))
    (property "Descriptions" "TVS 35.7V 7.5A SMA" (id 7) (at 200.66 36.83 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 180.34 102.87 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP14" (id 0) (at 178.943 100.809 0))
    (property "Value" "TestPoint_Small" (id 1) (at 180.34 104.902 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 175.26 102.87 0))
    (property "Datasheet" "~" (id 3) (at 175.26 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 144.78 132.08 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R107" (id 0) (at 146.558 131.1715 0))
    (property "Value" "30k" (id 1) (at 146.558 133.9466 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 146.558 132.08 90))
    (property "Datasheet" "~" (id 3) (at 144.78 132.08 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 144.78 132.08 0))
    (property "Description" "RES 30K 1% 1/10W 0603" (id 5) (at 144.78 132.08 0))
    (property "Manufacturer Product Number" "AECR0603F30K0K9" (id 6) (at 144.78 132.08 0))
    (property "Descriptions" "RES 30K 1% 1/10W 0603" (id 7) (at 144.78 132.08 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_2") (lib_id "Device:C") (at 95.25 110.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C105" (id 0) (at 96.901 108.3115 0))
    (property "Value" "10nF/100V" (id 1) (at 91.821 116.1666 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 96.2152 114.3 0))
    (property "Datasheet" "~" (id 3) (at 95.25 110.49 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB103" (id 4) (at 95.25 110.49 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 95.25 110.49 0))
    (property "Description" "CAP CER 10nF 100V X7R 0603" (id 6) (at 95.25 110.49 0))
    (property "Descriptions" "CAP CER 10nF 100V X7R 0603" (id 7) (at 95.25 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 52.07 149.86 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R103" (id 0) (at 53.848 148.9515 0))
    (property "Value" "30k" (id 1) (at 53.848 151.7266 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 53.848 149.86 90))
    (property "Datasheet" "~" (id 3) (at 52.07 149.86 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 52.07 149.86 0))
    (property "Description" "RES 30K 1% 1/10W 0603" (id 5) (at 52.07 149.86 0))
    (property "Manufacturer Product Number" "AECR0603F30K0K9" (id 6) (at 52.07 149.86 0))
    (property "Descriptions" "RES 30K 1% 1/10W 0603" (id 7) (at 52.07 149.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 83.82 119.38 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP10" (id 0) (at 84.963 119.859 0))
    (property "Value" "TestPoint_Small" (id 1) (at 83.82 121.412 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 78.74 119.38 0))
    (property "Datasheet" "~" (id 3) (at 78.74 119.38 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 78.74 110.49 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP11" (id 0) (at 76.073 112.239 0))
    (property "Value" "TestPoint_Small" (id 1) (at 78.74 112.522 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 73.66 110.49 0))
    (property "Datasheet" "~" (id 3) (at 73.66 110.49 0))
    (pin "1")
  )
  (symbol (lib_name "C_4") (lib_id "Device:C") (at 152.4 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C107" (id 0) (at 152.781 107.0415 0))
    (property "Value" "100nF/100V" (id 1) (at 148.971 116.1666 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 153.3652 113.03 0))
    (property "Datasheet" "~" (id 3) (at 152.4 109.22 0))
    (property "Manufacturer Product Number" "AC0805KKX7R0BB104" (id 4) (at 152.4 109.22 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 152.4 109.22 0))
    (property "Description" "CAP CER 0.1uF 100V X7R 0805" (id 6) (at 152.4 109.22 0))
    (property "Descriptions" "CAP CER 0.1uF 100V X7R 0805" (id 7) (at 152.4 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 144.78 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R108" (id 0) (at 146.558 143.8715 0))
    (property "Value" "10k" (id 1) (at 146.558 146.6466 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 143.002 144.78 90))
    (property "Datasheet" "~" (id 3) (at 144.78 144.78 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 144.78 144.78 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 144.78 144.78 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 144.78 144.78 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 144.78 144.78 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 41.91 125.73 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R101" (id 0) (at 41.91 120.7475 90))
    (property "Value" "10k" (id 1) (at 41.91 123.5226 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 41.91 127.508 90))
    (property "Datasheet" "~" (id 3) (at 41.91 125.73 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 41.91 125.73 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 41.91 125.73 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 41.91 125.73 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 41.91 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 35.56 125.73 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP2" (id 0) (at 34.163 127.479 0))
    (property "Value" "TestPoint_Small" (id 1) (at 35.56 127.762 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 30.48 125.73 0))
    (property "Datasheet" "~" (id 3) (at 30.48 125.73 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 83.82 115.57 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R106" (id 0) (at 85.598 114.6615 0))
    (property "Value" "10k" (id 1) (at 85.598 117.4366 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 82.042 115.57 90))
    (property "Datasheet" "~" (id 3) (at 83.82 115.57 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 83.82 115.57 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 83.82 115.57 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 83.82 115.57 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 83.82 115.57 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 189.23 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0114" (id 0) (at 189.23 106.68 0))
    (property "Value" "+5V" (id 1) (at 189.23 99.2655 0))
    (property "Footprint" "" (id 2) (at 189.23 102.87 0))
    (property "Datasheet" "" (id 3) (at 189.23 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 48.26 102.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP4" (id 0) (at 46.863 100.809 0))
    (property "Value" "TestPoint_Small" (id 1) (at 48.26 100.838 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 53.34 102.87 0))
    (property "Datasheet" "~" (id 3) (at 53.34 102.87 0))
    (pin "1")
  )
  (symbol (lib_name "C_7") (lib_id "Device:C") (at 137.16 143.51 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C106" (id 0) (at 138.811 141.3315 0))
    (property "Value" "100nF/50V" (id 1) (at 132.461 146.6466 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 138.1252 147.32 0))
    (property "Datasheet" "~" (id 3) (at 137.16 143.51 0))
    (property "Manufacturer Product Number" " AC0603KRX7R9BB104" (id 4) (at 137.16 143.51 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 137.16 143.51 0))
    (property "Description" "CAP CER 100nF 50V X7R 0603" (id 6) (at 137.16 143.51 0))
    (property "Descriptions" "CAP CER 100nF 50V X7R 0603" (id 7) (at 137.16 143.51 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_4") (lib_id "Device:C") (at 38.1 110.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C101" (id 0) (at 32.131 108.3115 0))
    (property "Value" "100nF/100V" (id 1) (at 24.511 113.6266 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric" (id 2) (at 39.0652 114.3 0))
    (property "Datasheet" "~" (id 3) (at 38.1 110.49 0))
    (property "Manufacturer Product Number" "AC0805KKX7R0BB104" (id 4) (at 38.1 110.49 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 38.1 110.49 0))
    (property "Description" "CAP CER 0.1uF 100V X7R 0805" (id 6) (at 38.1 110.49 0))
    (property "Descriptions" "CAP CER 0.1uF 100V X7R 0805" (id 7) (at 38.1 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 219.71 29.21 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP17" (id 0) (at 220.853 29.689 0))
    (property "Value" "TestPoint_Small" (id 1) (at 219.71 31.242 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 214.63 29.21 0))
    (property "Datasheet" "~" (id 3) (at 214.63 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "Transistor_BJT:BCP53") (at 83.82 105.41 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q102" (id 0) (at 83.82 97.354 90))
    (property "Value" "BCP53TA" (id 1) (at 83.82 100.1291 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (id 2) (at 81.915 100.33 0))
    (property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/BCP53T1-D.PDF" (id 3) (at 83.82 105.41 0))
    (property "Description" "TRANS PNP 80V 1A SOT223-4" (id 4) (at 83.82 105.41 90))
    (property "Manufacturer" "Diodes" (id 5) (at 83.82 105.41 90))
    (property "Manufacturer Product Number" "BCP53TA" (id 6) (at 83.82 105.41 90))
    (property "Descriptions" "TRANS PNP 80V 1A SOT223-4" (id 7) (at 83.82 105.41 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:R") (at 43.18 140.97 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R102" (id 0) (at 43.18 135.9875 90))
    (property "Value" "30k" (id 1) (at 43.18 138.7626 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 43.18 142.748 90))
    (property "Datasheet" "~" (id 3) (at 43.18 140.97 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 43.18 140.97 0))
    (property "Description" "RES 30K 1% 1/10W 0603" (id 5) (at 43.18 140.97 0))
    (property "Manufacturer Product Number" "AECR0603F30K0K9" (id 6) (at 43.18 140.97 0))
    (property "Descriptions" "RES 30K 1% 1/10W 0603" (id 7) (at 43.18 140.97 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_7") (lib_id "Device:C") (at 44.45 161.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C102" (id 0) (at 38.481 159.1115 0))
    (property "Value" "100nF/50V" (id 1) (at 39.751 164.4266 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 45.4152 165.1 0))
    (property "Datasheet" "~" (id 3) (at 44.45 161.29 0))
    (property "Manufacturer Product Number" " AC0603KRX7R9BB104" (id 4) (at 44.45 161.29 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 44.45 161.29 0))
    (property "Description" "CAP CER 100nF 50V X7R 0603" (id 6) (at 44.45 161.29 0))
    (property "Descriptions" "CAP CER 100nF 50V X7R 0603" (id 7) (at 44.45 161.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 38.1 114.3 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0104" (id 0) (at 38.1 120.65 0))
    (property "Value" "GND" (id 1) (at 38.1 118.8624 0))
    (property "Footprint" "" (id 2) (at 38.1 114.3 0))
    (property "Datasheet" "" (id 3) (at 38.1 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 52.07 157.48 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP7" (id 0) (at 48.133 155.419 0))
    (property "Value" "TestPoint_Small" (id 1) (at 52.07 159.512 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 46.99 157.48 0))
    (property "Datasheet" "~" (id 3) (at 46.99 157.48 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_NPN_BEC_BRT") (at 82.55 133.35 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q101" (id 0) (at 86.1313 132.4415 0))
    (property "Value" "DDTC114ECA-7-F|PDTC114ET,215" (id 1) (at 86.1313 135.2166 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 82.55 133.35 0))
    (property "Datasheet" "~" (id 3) (at 82.55 133.35 0))
    (property "Manufacturer" "Diodes" (id 4) (at 82.55 133.35 0))
    (property "Manufacturer Product Number" "DDTC114ECA-7-F" (id 5) (at 82.55 133.35 0))
    (property "Description" "TRANS PREBIAS NPN 200MW SOT23-3" (id 6) (at 82.55 133.35 0))
    (property "Descriptions" "TRANS PREBIAS NPN 200MW SOT23-3" (id 7) (at 82.55 133.35 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+5V") (at 60.96 166.37 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 60.96 162.56 0))
    (property "Value" "+5V" (id 1) (at 59.69 171.45 0))
    (property "Footprint" "" (id 2) (at 60.96 166.37 0))
    (property "Datasheet" "" (id 3) (at 60.96 166.37 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_TVS") (at 48.26 110.49 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D102" (id 0) (at 50.292 109.5815 90))
    (property "Value" "SMAJ33CA-AT" (id 1) (at 50.292 112.3566 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 48.26 110.49 0))
    (property "Datasheet" "~" (id 3) (at 48.26 110.49 0))
    (property "Manufacturer Product Number" "SMAJ33CA-AT" (id 4) (at 48.26 110.49 90))
    (property "Manufacturer" "" (id 5) (at 48.26 110.49 90))
    (property "Description" "TVS 35.7V 7.5A SMA" (id 6) (at 48.26 110.49 0))
    (property "Descriptions" "TVS 35.7V 7.5A SMA" (id 7) (at 48.26 110.49 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Ferrite") (at 62.23 157.48 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L101" (id 0) (at 62.23 152.1164 90))
    (property "Value" "1k@100MHz" (id 1) (at 62.23 154.8915 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 62.23 157.48 0))
    (property "Datasheet" "~" (id 3) (at 62.23 157.48 0))
    (property "Manufacturer Product Number" "BLM18RK102SN1D" (id 4) (at 62.23 157.48 90))
    (property "Manufacturer" "Murata Electronics" (id 5) (at 62.23 157.48 90))
    (property "Description" "FERRITEBEAD SMD AUTOMOTIVE POWER" (id 6) (at 62.23 157.48 90))
    (property "Descriptions" "FERRITEBEAD SMD AUTOMOTIVE POWER" (id 7) (at 62.23 157.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_9") (lib_id "Device:C") (at 180.34 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C108" (id 0) (at 181.991 107.0415 0))
    (property "Value" "10uF/10V" (id 1) (at 176.911 113.6266 90))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric" (id 2) (at 181.3052 113.03 0))
    (property "Datasheet" "~" (id 3) (at 180.34 109.22 0))
    (property "Manufacturer Product Number" "CC1206KKX7R6BB106" (id 4) (at 180.34 109.22 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 180.34 109.22 0))
    (property "Description" "CAP CER 10UF 10V X7R 1206" (id 6) (at 180.34 109.22 0))
    (property "Descriptions" "CAP CER 10UF 10V X7R 1206" (id 7) (at 180.34 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_8") (lib_id "Device:C") (at 196.85 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C111" (id 0) (at 198.501 107.0415 0))
    (property "Value" "1nF/50V" (id 1) (at 198.501 112.3566 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 197.8152 113.03 0))
    (property "Datasheet" "~" (id 3) (at 196.85 109.22 0))
    (property "Manufacturer Product Number" "AC0603KRX7R9BB102" (id 4) (at 196.85 109.22 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 196.85 109.22 0))
    (property "Description" "CAP CER 1000PF 50V X7R 0603" (id 6) (at 196.85 109.22 0))
    (property "Descriptions" "CAP CER 1000PF 50V X7R 0603" (id 7) (at 196.85 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 166.37 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0112" (id 0) (at 166.37 124.46 0))
    (property "Value" "GND" (id 1) (at 166.37 122.6724 0))
    (property "Footprint" "" (id 2) (at 166.37 118.11 0))
    (property "Datasheet" "" (id 3) (at 166.37 118.11 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 170.18 148.59 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR05" (id 0) (at 170.18 154.94 0))
    (property "Value" "GND" (id 1) (at 170.18 153.1524 0))
    (property "Footprint" "" (id 2) (at 170.18 148.59 0))
    (property "Datasheet" "" (id 3) (at 170.18 148.59 0))
    (pin "1")
  )
  (symbol (lib_id "Regulator_Linear:MCP1703A-1202_SOT223") (at 166.37 102.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U101" (id 0) (at 166.37 96.9984 0))
    (property "Value" "BD450M2FP3-CE2" (id 1) (at 166.37 99.7735 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (id 2) (at 166.37 97.79 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005122B.pdf" (id 3) (at 166.37 104.14 0))
    (property "Manufacturer" "Rohm Semiconductor" (id 4) (at 166.37 102.87 0))
    (property "Manufacturer Product Number" "BD450M2FP3-CE2" (id 5) (at 166.37 102.87 0))
    (property "Description" "IC REG LINEAR 5V 200MA SOT223-4F" (id 6) (at 166.37 102.87 0))
    (property "Descriptions" "IC REG LINEAR 5V 200MA SOT223-4F" (id 7) (at 166.37 102.87 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_name "C_1") (lib_id "Device:C") (at 137.16 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C103" (id 0) (at 138.811 107.0415 0))
    (property "Value" "4.7uF/50V" (id 1) (at 133.731 114.8966 90))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric" (id 2) (at 138.1252 113.03 0))
    (property "Datasheet" "~" (id 3) (at 137.16 109.22 0))
    (property "Manufacturer Product Number" "CC1206KKX7R9BB475" (id 4) (at 137.16 109.22 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 137.16 109.22 0))
    (property "Description" "CAP CER 4.7uF 50V X7R 1206" (id 6) (at 137.16 109.22 0))
    (property "Descriptions" "CAP CER 4.7uF 50V X7R 1206" (id 7) (at 137.16 109.22 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 193.04 29.21 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP16" (id 0) (at 194.183 29.689 0))
    (property "Value" "TestPoint_Small" (id 1) (at 193.04 31.242 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 187.96 29.21 0))
    (property "Datasheet" "~" (id 3) (at 187.96 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 144.78 148.59 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0111" (id 0) (at 144.78 154.94 0))
    (property "Value" "GND" (id 1) (at 144.78 153.1524 0))
    (property "Footprint" "" (id 2) (at 144.78 148.59 0))
    (property "Datasheet" "" (id 3) (at 144.78 148.59 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 62.23 133.35 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP8" (id 0) (at 60.833 135.099 0))
    (property "Value" "TestPoint_Small" (id 1) (at 62.23 135.382 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 57.15 133.35 0))
    (property "Datasheet" "~" (id 3) (at 57.15 133.35 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 68.58 157.48 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP9" (id 0) (at 67.183 160.499 0))
    (property "Value" "TestPoint_Small" (id 1) (at 68.58 159.512 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 63.5 157.48 0))
    (property "Datasheet" "~" (id 3) (at 63.5 157.48 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 182.88 45.72 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP15" (id 0) (at 184.023 46.199 0))
    (property "Value" "TestPoint_Small" (id 1) (at 182.88 47.752 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 177.8 45.72 0))
    (property "Datasheet" "~" (id 3) (at 177.8 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 137.16 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0110" (id 0) (at 137.16 124.46 0))
    (property "Value" "GND" (id 1) (at 137.16 122.6724 0))
    (property "Footprint" "" (id 2) (at 137.16 118.11 0))
    (property "Datasheet" "" (id 3) (at 137.16 118.11 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 71.12 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R105" (id 0) (at 72.898 105.7715 0))
    (property "Value" "51k" (id 1) (at 72.898 108.5466 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 69.342 106.68 90))
    (property "Datasheet" "~" (id 3) (at 71.12 106.68 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 71.12 106.68 0))
    (property "Description" "RES 51k 1% 1/10W 0603" (id 5) (at 71.12 106.68 0))
    (property "Manufacturer Product Number" "AECR0603F51K0K9" (id 6) (at 71.12 106.68 0))
    (property "Descriptions" "RES 51k 1% 1/10W 0603" (id 7) (at 71.12 106.68 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 182.88 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0113" (id 0) (at 182.88 54.61 0))
    (property "Value" "GND" (id 1) (at 182.88 52.8224 0))
    (property "Footprint" "" (id 2) (at 182.88 48.26 0))
    (property "Datasheet" "" (id 3) (at 182.88 48.26 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:BAV99S") (at 68.58 166.37 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D2" (id 0) (at 67.31 170.18 0))
    (property "Value" "BAV99S,115" (id 1) (at 67.31 172.72 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 68.58 153.67 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf" (id 3) (at 68.58 166.37 0))
    (property "Descriptions" "DIODE ARRAY GP 100V 200MA 6TSSOP" (id 4) (at 68.58 166.37 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 83.82 124.46 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D3" (id 0) (at 86.36 123.5074 90))
    (property "Value" "BAS316" (id 1) (at 85.09 127 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 83.82 124.46 0))
    (property "Datasheet" "~" (id 3) (at 83.82 124.46 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 83.82 124.46 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 83.82 124.46 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 83.82 124.46 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D") (at 35.56 140.97 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D101" (id 0) (at 35.56 135.7335 0))
    (property "Value" "BAS16" (id 1) (at 35.56 138.5086 0))
    (property "Footprint" "Diode_SMD:D_SOD-123" (id 2) (at 35.56 140.97 0))
    (property "Datasheet" "~" (id 3) (at 35.56 140.97 0))
    (property "Manufacturer" "Nexperia(安世)" (id 4) (at 35.56 140.97 0))
    (property "Manufacturer Product Number" "BAS16GW" (id 5) (at 35.56 140.97 0))
    (property "Description" "DIODE GEN PURP 100V 215MA SOD123" (id 7) (at 35.56 140.97 0))
    (property "Descriptions" "DIODE GEN PURP 100V 215MA SOD123" (id 8) (at 35.56 140.97 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 48.26 125.73 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP5" (id 0) (at 48.133 123.669 0))
    (property "Value" "TestPoint_Small" (id 1) (at 48.26 127.762 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 43.18 125.73 0))
    (property "Datasheet" "~" (id 3) (at 43.18 125.73 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 76.2 166.37 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR03" (id 0) (at 82.55 166.37 0))
    (property "Value" "GND" (id 1) (at 80.01 166.3699 90))
    (property "Footprint" "" (id 2) (at 76.2 166.37 0))
    (property "Datasheet" "" (id 3) (at 76.2 166.37 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 52.07 144.78 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "TP6" (id 0) (at 53.213 145.259 0))
    (property "Value" "TestPoint_Small" (id 1) (at 52.07 146.812 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 46.99 144.78 0))
    (property "Datasheet" "~" (id 3) (at 46.99 144.78 0))
    (pin "1")
  )
  (symbol (lib_name "C_2") (lib_id "Device:C") (at 217.17 36.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C112" (id 0) (at 218.821 34.6515 0))
    (property "Value" "10nF/100V" (id 1) (at 225.171 42.5066 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 218.1352 40.64 0))
    (property "Datasheet" "~" (id 3) (at 217.17 36.83 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB103" (id 4) (at 217.17 36.83 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 217.17 36.83 0))
    (property "Description" "CAP CER 10nF 100V X7R 0603" (id 6) (at 217.17 36.83 0))
    (property "Descriptions" "CAP CER 10nF 100V X7R 0603" (id 7) (at 217.17 36.83 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 52.07 162.56 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R104" (id 0) (at 53.848 161.6515 0))
    (property "Value" "10k" (id 1) (at 53.848 164.4266 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 50.292 162.56 90))
    (property "Datasheet" "~" (id 3) (at 52.07 162.56 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 52.07 162.56 0))
    (property "Description" "RES 10k 1% 1/10W 0603" (id 5) (at 52.07 162.56 0))
    (property "Manufacturer Product Number" "AECR0603F10K0K9" (id 6) (at 52.07 162.56 0))
    (property "Descriptions" "RES 10k 1% 1/10W 0603" (id 7) (at 52.07 162.56 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 115.57 116.84 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0108" (id 0) (at 115.57 123.19 0))
    (property "Value" "GND" (id 1) (at 115.57 121.4024 0))
    (property "Footprint" "" (id 2) (at 115.57 116.84 0))
    (property "Datasheet" "" (id 3) (at 115.57 116.84 0))
    (pin "1")
  )
)
