(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "SX7H SHIFER MIAN SCH")
    (date "2022-07-18")
    (rev "V03")
    (company "宁波正朗汽车零部件有限公司")
    (comment 1 "批准:")
    (comment 2 "校准：")
    (comment 3 "设计：Ethan")
  )
  (lib_symbols
    (symbol "C_6" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_6" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 4) (at 0 0 0))
      (property "Manufacturer" "" (id 5) (at 0 0 0))
      (property "Description" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 7) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 9) (at 0 0 0))
      (symbol "C_6_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_6_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Connector:TestPoint_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 3.81 0))
      (property "Value" "TestPoint_Small" (id 1) (at 0 2.032 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_Small_0_1"
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "TestPoint_Small_1_1"
        (pin passive line (at 0 0 90) (length 0)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Device:D_Schottky_Filled" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D_Schottky_Filled" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "Schottky diode, filled shape" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_Schottky_Filled_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "D_Schottky_Filled_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:D_TVS_Dual_AAC" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 4.445 0))
      (property "Value" "D_TVS_Dual_AAC" (id 1) (at 0 2.54 0))
      (property "Footprint" "" (id 2) (at -3.81 0 0))
      (property "Datasheet" "~" (id 3) (at -3.81 0 0))
      (property "ki_keywords" "diode TVS thyrector" (id 4) (at 0 0 0))
      (property "ki_description" "Bidirectional dual transient-voltage-suppression diode, center on pin 3" (id 5) (at 0 0 0))
      (symbol "D_TVS_Dual_AAC_0_0"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 0)
          )
          (fill (type none))
        )
      )
      (symbol "D_TVS_Dual_AAC_0_1"
        (polyline
          (pts
            (xy -6.35 0)
            (xy 6.35 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.302 1.27)
            (xy -3.81 1.27)
            (xy -3.81 -1.27)
            (xy -4.318 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 1.27)
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.302 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 1.27)
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -6.35 -1.27)
            (xy -6.35 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.35 1.27)
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 6.35 -1.27)
            (xy 6.35 1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "D_TVS_Dual_AAC_1_1"
        (pin passive line (at -8.89 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 8.89 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "common")
          (number "3")
        )
      )
    )
    (symbol "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 3.81 1.27 0))
      (property "Value" "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor NPN" (id 4) (at 0 0 0))
      (property "ki_description" "Dual NPN/PNP bias resistor transistor, 6 pin package" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SC?70* SC?88* SOT*363*" (id 6) (at 0 0 0))
      (symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_0_1"
        (rectangle (start -6.35 0.508) (end -4.826 -0.508)
          (fill (type none))
        )
        (rectangle (start -4.318 -2.286) (end -3.302 -0.762)
          (fill (type none))
        )
        (circle (center -3.81 0) (radius 0.254)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -3.81 -0.762)
            (xy -3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 0)
            (xy -4.826 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 1.524)
            (xy -0.635 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -2.286)
            (xy -3.81 -3.048)
            (xy 1.27 -3.048)
          )
          (fill (type none))
        )
        (circle (center 1.27 -3.048) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_1_1"
        (polyline
          (pts
            (xy -0.635 0.635)
            (xy 1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -0.635)
            (xy 1.27 -2.54)
            (xy 1.27 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.778)
            (xy 0.508 -1.27)
            (xy 1.016 -2.286)
            (xy 0 -1.778)
            (xy 0 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 0 0) (radius 2.8194)
          (fill (type none))
        )
        (pin passive line (at 1.27 -5.08 90) (length 2.54)
          (name "E1")
          (number "1")
        )
        (pin input line (at -8.89 0 0) (length 2.54)
          (name "B1")
          (number "2")
        )
        (pin passive line (at 1.27 5.08 270) (length 2.54)
          (name "C1")
          (number "6")
        )
      )
      (symbol "Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1_2_1"
        (polyline
          (pts
            (xy -0.635 0.635)
            (xy 1.27 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 -0.635)
            (xy 1.27 -2.54)
            (xy 1.27 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.778)
            (xy 0.508 -2.286)
            (xy 0 -1.27)
            (xy 1.016 -1.778)
            (xy 1.016 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 0 0) (radius 2.8194)
          (fill (type none))
        )
        (pin passive line (at 1.27 5.08 270) (length 2.54)
          (name "C1")
          (number "3")
        )
        (pin passive line (at 1.27 -5.08 90) (length 2.54)
          (name "E1")
          (number "4")
        )
        (pin input line (at -8.89 0 0) (length 2.54)
          (name "B1")
          (number "5")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Manufacturer" "" (id 4) (at 0 0 0))
      (property "Description" "" (id 5) (at 0 0 0))
      (property "Manufacturer Product Number" "" (id 6) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 7) (at 0 0 0))
      (property "ki_description" "Resistor" (id 8) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 9) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "power:+12P" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+12P" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+12P\"" (id 5) (at 0 0 0))
      (symbol "+12P_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+12P_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+12P")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 232.41 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 241.6842 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 225.9339 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 240.03 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 241.3 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 224.79 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 167.64 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 229.87 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 234.95 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 236.0066 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 31.75) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 101.6 71.12) (xy 101.6 73.66)))
  (wire (pts (xy 255.27 142.24) (xy 255.27 143.51)))
  (wire (pts (xy 163.83 73.66) (xy 167.64 73.66)))
  (wire (pts (xy 256.54 74.93) (xy 262.89 74.93)))
  (wire (pts (xy 236.22 31.75) (xy 240.03 31.75)))
  (wire (pts (xy 240.03 31.75) (xy 245.11 31.75)))
  (wire (pts (xy 229.87 114.3) (xy 233.68 114.3)))
  (wire (pts (xy 182.88 73.66) (xy 189.23 73.66)))
  (wire (pts (xy 101.6 49.53) (xy 110.49 49.53)))
  (wire (pts (xy 241.3 74.93) (xy 241.6842 74.93)))
  (wire (pts (xy 260.35 114.3) (xy 266.7 114.3)))
  (wire (pts (xy 101.6 31.75) (xy 110.49 31.75)))
  (wire (pts (xy 149.86 31.75) (xy 153.67 31.75)))
  (wire (pts (xy 241.3 114.3) (xy 245.11 114.3)))
  (wire (pts (xy 245.11 114.3) (xy 250.19 114.3)))
  (wire (pts (xy 175.26 59.69) (xy 175.26 60.96)))
  (wire (pts (xy 161.29 31.75) (xy 165.1 31.75)))
  (wire (pts (xy 165.1 31.75) (xy 170.18 31.75)))
  (wire (pts (xy 223.52 97.79) (xy 234.95 97.79)))
  (wire (pts (xy 234.95 97.79) (xy 241.3 97.79)))
  (wire (pts (xy 241.6842 74.93) (xy 246.38 74.93)))
  (wire (pts (xy 147.32 31.75) (xy 149.86 31.75)))
  (wire (pts (xy 149.86 96.52) (xy 160.02 96.52)))
  (wire (pts (xy 160.02 96.52) (xy 167.64 96.52)))
  (wire (pts (xy 101.6 53.34) (xy 110.49 53.34)))
  (wire (pts (xy 227.33 137.16) (xy 236.0066 137.16)))
  (wire (pts (xy 236.0066 137.16) (xy 245.11 137.16)))
  (wire (pts (xy 223.52 74.93) (xy 225.9339 74.93)))
  (wire (pts (xy 177.8 101.6) (xy 177.8 102.87)))
  (wire (pts (xy 101.6 73.66) (xy 110.49 73.66)))
  (wire (pts (xy 250.19 59.69) (xy 250.19 60.96)))
  (wire (pts (xy 251.46 102.87) (xy 251.46 104.14)))
  (wire (pts (xy 101.6 95.25) (xy 110.49 95.25)))
  (wire (pts (xy 237.49 74.93) (xy 241.3 74.93)))
  (wire (pts (xy 255.27 31.75) (xy 261.62 31.75)))
  (wire (pts (xy 224.79 31.75) (xy 228.6 31.75)))
  (wire (pts (xy 225.9339 74.93) (xy 229.87 74.93)))
  (wire (pts (xy 167.64 73.66) (xy 172.72 73.66)))
  (wire (pts (xy 222.25 31.75) (xy 224.79 31.75)))
  (wire (pts (xy 147.32 54.61) (xy 162.56 54.61)))
  (wire (pts (xy 162.56 54.61) (xy 165.1 54.61)))
  (wire (pts (xy 149.86 73.66) (xy 152.4 73.66)))
  (wire (pts (xy 152.4 73.66) (xy 156.21 73.66)))
  (wire (pts (xy 222.25 54.61) (xy 232.41 54.61)))
  (wire (pts (xy 232.41 54.61) (xy 240.03 54.61)))
  (wire (pts (xy 227.33 114.3) (xy 229.87 114.3)))
  (wire (pts (xy 180.34 31.75) (xy 186.69 31.75)))
  (wire (pts (xy 101.6 77.47) (xy 110.49 77.47)))
  (label "N_LED_O" (at 105.41 73.66 0))
  (label "N_LED_O" (at 229.87 114.3 0))
  (label "D_LED_O" (at 224.79 31.75 0))
  (label "R_LED_O" (at 102.87 53.34 0))
  (label "P_LED_O" (at 104.14 31.75 0))
  (label "M_LED_O" (at 152.4 73.66 0))
  (label "D_LED_O" (at 105.41 77.47 0))
  (label "P_LED_O" (at 149.86 31.75 0))
  (label "M_LED_O" (at 105.41 95.25 0))
  (label "P_LED_O" (at 102.87 49.53 0))
  (label "R_LED_O" (at 226.06 74.93 0))
  (hierarchical_label "N_LED_OH" (shape input) (at 227.33 114.3 180))
  (hierarchical_label "P_LED_C" (shape input) (at 147.32 54.61 180))
  (hierarchical_label "M_LED_C" (shape input) (at 149.86 96.52 180))
  (hierarchical_label "Paddle-_AI" (shape input) (at 118.11 74.93 0))
  (hierarchical_label "M_LED_OH" (shape input) (at 149.86 73.66 180))
  (hierarchical_label "Paddle+_AI" (shape input) (at 118.11 34.29 0))
  (hierarchical_label "D_LED_C" (shape input) (at 222.25 54.61 180))
  (hierarchical_label "R_LED_OH" (shape input) (at 223.52 74.93 180))
  (hierarchical_label "N_LED_C" (shape input) (at 227.33 137.16 180))
  (hierarchical_label "R_LED_C" (shape input) (at 223.52 97.79 180))
  (hierarchical_label "D_LED_OH" (shape input) (at 222.25 31.75 180))
  (hierarchical_label "P_LED_OH" (shape input) (at 147.32 31.75 180))
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 176.53 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q104" (id 0) (at 180.1113 95.6115 0))
    (property "Value" "PUMD3,115" (id 1) (at 180.1113 98.3866 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 176.53 96.52 0))
    (property "Datasheet" "~" (id 3) (at 176.53 96.52 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 176.53 96.52 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 176.53 96.52 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 176.53 96.52 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 176.53 96.52 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 255.27 115.57 90) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q107" (id 0) (at 255.27 108.784 90))
    (property "Value" "PUMD3,115" (id 1) (at 255.27 111.5591 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 255.27 115.57 0))
    (property "Datasheet" "~" (id 3) (at 255.27 115.57 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 255.27 115.57 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 255.27 115.57 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 255.27 115.57 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 255.27 115.57 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 229.87 114.3 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP79" (id 0) (at 228.473 112.239 0))
    (property "Value" "TestPoint_Small" (id 1) (at 229.87 116.332 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 224.79 114.3 0))
    (property "Datasheet" "~" (id 3) (at 224.79 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12P") (at 266.7 114.3 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0175" (id 0) (at 262.89 114.3 0))
    (property "Value" "+12P" (id 1) (at 269.8749 114.779 90))
    (property "Footprint" "" (id 2) (at 266.7 114.3 0))
    (property "Datasheet" "" (id 3) (at 266.7 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 157.48 31.75 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R143" (id 0) (at 157.48 26.7675 90))
    (property "Value" "1.1k" (id 1) (at 157.48 29.5426 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 157.48 33.528 90))
    (property "Datasheet" "~" (id 3) (at 157.48 31.75 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 157.48 31.75 0))
    (property "Description" "RES 1k 1% 1/4W 1206" (id 5) (at 157.48 31.75 0))
    (property "Manufacturer Product Number" "AECR1206F1K10K9" (id 6) (at 157.48 31.75 0))
    (property "Descriptions" "RES 1.1k 1% 1/4W 1206" (id 7) (at 157.48 31.75 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 236.0066 137.16 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP82" (id 0) (at 234.6096 138.909 0))
    (property "Value" "TestPoint_Small" (id 1) (at 236.0066 139.192 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 230.9266 137.16 0))
    (property "Datasheet" "~" (id 3) (at 230.9266 137.16 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 245.11 121.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0169" (id 0) (at 245.11 128.27 0))
    (property "Value" "GND" (id 1) (at 245.11 125.73 0))
    (property "Footprint" "" (id 2) (at 245.11 121.92 0))
    (property "Datasheet" "" (id 3) (at 245.11 121.92 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 251.46 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0171" (id 0) (at 251.46 110.49 0))
    (property "Value" "GND" (id 1) (at 251.46 108.7024 0))
    (property "Footprint" "" (id 2) (at 251.46 104.14 0))
    (property "Datasheet" "" (id 3) (at 251.46 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 173.99 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q103" (id 0) (at 177.5713 53.7015 0))
    (property "Value" "PUMD3,115" (id 1) (at 177.5713 56.4766 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 173.99 54.61 0))
    (property "Datasheet" "~" (id 3) (at 173.99 54.61 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 173.99 54.61 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 173.99 54.61 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 173.99 54.61 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 173.99 54.61 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 225.9339 74.93 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP78" (id 0) (at 224.5369 72.869 0))
    (property "Value" "TestPoint_Small" (id 1) (at 225.9339 76.962 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 220.8539 74.93 0))
    (property "Datasheet" "~" (id 3) (at 220.8539 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 251.46 76.2 90) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q106" (id 0) (at 251.46 69.414 90))
    (property "Value" "PUMD3,115" (id 1) (at 251.46 72.1891 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 251.46 76.2 0))
    (property "Datasheet" "~" (id 3) (at 251.46 76.2 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 251.46 76.2 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 251.46 76.2 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 251.46 76.2 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 251.46 76.2 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 97.79 40.64 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR06" (id 0) (at 91.44 40.64 0))
    (property "Value" "GND" (id 1) (at 99.06 40.6399 90))
    (property "Footprint" "" (id 2) (at 97.79 40.64 0))
    (property "Datasheet" "" (id 3) (at 97.79 40.64 0))
    (pin "1")
  )
  (symbol (lib_name "C_6") (lib_id "Device:C") (at 245.11 118.11 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C143" (id 0) (at 237.49 118.11 0))
    (property "Value" "47nF{slash}100V" (id 1) (at 232.41 121.92 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 246.0752 121.92 0))
    (property "Datasheet" "~" (id 3) (at 245.11 118.11 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB473" (id 4) (at 245.11 118.11 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 245.11 118.11 0))
    (property "Description" "CAP CER 47nF 100V X7R 0603" (id 6) (at 245.11 118.11 0))
    (property "Descriptions" "CAP CER 47nF 100V X7R 0603" (id 7) (at 245.11 118.11 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 167.64 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0162" (id 0) (at 167.64 87.63 0))
    (property "Value" "GND" (id 1) (at 167.64 85.09 0))
    (property "Footprint" "" (id 2) (at 167.64 81.28 0))
    (property "Datasheet" "" (id 3) (at 167.64 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 254 137.16 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q107" (id 0) (at 257.5813 136.2515 0))
    (property "Value" "PUMD3,115" (id 1) (at 257.5813 139.0266 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 254 137.16 0))
    (property "Datasheet" "~" (id 3) (at 254 137.16 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 254 137.16 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 254 137.16 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 254 137.16 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 254 137.16 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 177.8 87.63 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D7" (id 0) (at 180.34 86.6774 90))
    (property "Value" "BAS316" (id 1) (at 179.07 90.17 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 177.8 87.63 0))
    (property "Datasheet" "~" (id 3) (at 177.8 87.63 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 177.8 87.63 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 177.8 87.63 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 177.8 87.63 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 234.95 97.79 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP81" (id 0) (at 233.553 99.539 0))
    (property "Value" "TestPoint_Small" (id 1) (at 234.95 99.822 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 229.87 97.79 0))
    (property "Datasheet" "~" (id 3) (at 229.87 97.79 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 160.02 96.52 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP71" (id 0) (at 159.893 98.269 0))
    (property "Value" "TestPoint_Small" (id 1) (at 160.02 98.552 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 154.94 96.52 0))
    (property "Datasheet" "~" (id 3) (at 154.94 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 250.19 45.72 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D10" (id 0) (at 252.73 44.7674 90))
    (property "Value" "BAS316" (id 1) (at 251.46 48.26 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 250.19 45.72 0))
    (property "Datasheet" "~" (id 3) (at 250.19 45.72 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 250.19 45.72 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 250.19 45.72 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 250.19 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 240.03 31.75 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP83" (id 0) (at 238.633 29.689 0))
    (property "Value" "TestPoint_Small" (id 1) (at 240.03 33.782 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 234.95 31.75 0))
    (property "Datasheet" "~" (id 3) (at 234.95 31.75 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_TVS_Dual_AAC") (at 101.6 86.36 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D8" (id 0) (at 104.14 85.0899 90))
    (property "Value" "ESDA25L" (id 1) (at 104.14 87.6299 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 101.6 90.17 0))
    (property "Datasheet" "~" (id 3) (at 101.6 90.17 0))
    (property "Descriptions" "TVS DIODE 24VWM SOT23-3" (id 4) (at 101.6 86.36 0))
    (property "Manufacturer" "BORN(伯恩半导体)" (id 5) (at 101.6 86.36 0))
    (property "Manufacturer Product Number" " ESDA25L" (id 6) (at 101.6 86.36 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+12P") (at 261.62 31.75 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0173" (id 0) (at 257.81 31.75 0))
    (property "Value" "+12P" (id 1) (at 264.7949 32.229 90))
    (property "Footprint" "" (id 2) (at 261.62 31.75 0))
    (property "Datasheet" "" (id 3) (at 261.62 31.75 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 237.49 114.3 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R147" (id 0) (at 237.49 109.3175 90))
    (property "Value" "1.1k" (id 1) (at 237.49 112.0926 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 237.49 116.078 90))
    (property "Datasheet" "~" (id 3) (at 237.49 114.3 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 237.49 114.3 0))
    (property "Description" "RES 1k 1% 1/4W 1206" (id 5) (at 237.49 114.3 0))
    (property "Manufacturer Product Number" "AECR1206F1K10K9" (id 6) (at 237.49 114.3 0))
    (property "Descriptions" "RES 1.1k 1% 1/4W 1206" (id 7) (at 237.49 114.3 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 161.29 39.37 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0161" (id 0) (at 161.29 45.72 0))
    (property "Value" "GND" (id 1) (at 161.29 44.45 0))
    (property "Footprint" "" (id 2) (at 161.29 39.37 0))
    (property "Datasheet" "" (id 3) (at 161.29 39.37 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 167.64 73.66 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP74" (id 0) (at 166.243 71.599 0))
    (property "Value" "TestPoint_Small" (id 1) (at 167.64 75.692 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 162.56 73.66 0))
    (property "Datasheet" "~" (id 3) (at 162.56 73.66 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 255.27 128.27 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D12" (id 0) (at 257.81 127.3174 90))
    (property "Value" "BAS316" (id 1) (at 256.54 130.81 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 255.27 128.27 0))
    (property "Datasheet" "~" (id 3) (at 255.27 128.27 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 255.27 128.27 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 255.27 128.27 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 255.27 128.27 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D_TVS_Dual_AAC") (at 101.6 62.23 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D9" (id 0) (at 104.14 60.9599 90))
    (property "Value" "ESDA25L" (id 1) (at 104.14 63.4999 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 101.6 66.04 0))
    (property "Datasheet" "~" (id 3) (at 101.6 66.04 0))
    (property "Descriptions" "TVS DIODE 24VWM SOT23-3" (id 4) (at 101.6 62.23 0))
    (property "Manufacturer" "BORN(伯恩半导体)" (id 5) (at 101.6 62.23 0))
    (property "Manufacturer Product Number" " ESDA25L" (id 6) (at 101.6 62.23 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 251.46 88.9 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D11" (id 0) (at 254 87.9474 90))
    (property "Value" "BAS316" (id 1) (at 252.73 91.44 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 251.46 88.9 0))
    (property "Datasheet" "~" (id 3) (at 251.46 88.9 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 251.46 88.9 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 251.46 88.9 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 251.46 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 255.27 143.51 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0172" (id 0) (at 255.27 149.86 0))
    (property "Value" "GND" (id 1) (at 255.27 148.0724 0))
    (property "Footprint" "" (id 2) (at 255.27 143.51 0))
    (property "Datasheet" "" (id 3) (at 255.27 143.51 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 250.19 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0170" (id 0) (at 250.19 67.31 0))
    (property "Value" "GND" (id 1) (at 250.19 65.5224 0))
    (property "Footprint" "" (id 2) (at 250.19 60.96 0))
    (property "Datasheet" "" (id 3) (at 250.19 60.96 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 233.68 74.93 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R146" (id 0) (at 233.68 69.9475 90))
    (property "Value" "1.1k" (id 1) (at 233.68 72.7226 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 233.68 76.708 90))
    (property "Datasheet" "~" (id 3) (at 233.68 74.93 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 233.68 74.93 0))
    (property "Description" "RES 1k 1% 1/4W 1206" (id 5) (at 233.68 74.93 0))
    (property "Manufacturer Product Number" "AECR1206F1K10K9" (id 6) (at 233.68 74.93 0))
    (property "Descriptions" "RES 1.1k 1% 1/4W 1206" (id 7) (at 233.68 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 241.3 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0168" (id 0) (at 241.3 88.9 0))
    (property "Value" "GND" (id 1) (at 241.3 86.36 0))
    (property "Footprint" "" (id 2) (at 241.3 82.55 0))
    (property "Datasheet" "" (id 3) (at 241.3 82.55 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 240.03 39.37 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0167" (id 0) (at 240.03 45.72 0))
    (property "Value" "GND" (id 1) (at 240.03 43.9324 0))
    (property "Footprint" "" (id 2) (at 240.03 39.37 0))
    (property "Datasheet" "" (id 3) (at 240.03 39.37 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 160.02 73.66 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R144" (id 0) (at 160.02 68.6775 90))
    (property "Value" "1.1k" (id 1) (at 160.02 71.4526 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 160.02 75.438 90))
    (property "Datasheet" "~" (id 3) (at 160.02 73.66 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 160.02 73.66 0))
    (property "Description" "RES 1k 1% 1/4W 1206" (id 5) (at 160.02 73.66 0))
    (property "Manufacturer Product Number" "AECR1206F1K10K9" (id 6) (at 160.02 73.66 0))
    (property "Descriptions" "RES 1.1k 1% 1/4W 1206" (id 7) (at 160.02 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 232.41 54.61 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP80" (id 0) (at 232.283 56.359 0))
    (property "Value" "TestPoint_Small" (id 1) (at 232.41 56.642 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 227.33 54.61 0))
    (property "Datasheet" "~" (id 3) (at 227.33 54.61 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 175.26 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0163" (id 0) (at 175.26 67.31 0))
    (property "Value" "GND" (id 1) (at 175.26 65.5224 0))
    (property "Footprint" "" (id 2) (at 175.26 60.96 0))
    (property "Datasheet" "" (id 3) (at 175.26 60.96 0))
    (pin "1")
  )
  (symbol (lib_id "Device:D_TVS_Dual_AAC") (at 101.6 40.64 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D5" (id 0) (at 104.14 39.3699 90))
    (property "Value" "ESDA25L" (id 1) (at 104.14 41.9099 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 101.6 44.45 0))
    (property "Datasheet" "~" (id 3) (at 101.6 44.45 0))
    (property "Descriptions" "TVS DIODE 24VWM SOT23-3" (id 4) (at 101.6 40.64 0))
    (property "Manufacturer" "BORN(伯恩半导体)" (id 5) (at 101.6 40.64 0))
    (property "Manufacturer Product Number" " ESDA25L" (id 6) (at 101.6 40.64 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 232.41 31.75 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R145" (id 0) (at 232.41 26.7675 90))
    (property "Value" "1.1k" (id 1) (at 232.41 29.5426 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric" (id 2) (at 232.41 33.528 90))
    (property "Datasheet" "~" (id 3) (at 232.41 31.75 0))
    (property "Manufacturer" "RESI(开步睿思)" (id 4) (at 232.41 31.75 0))
    (property "Description" "RES 1k 1% 1/4W 1206" (id 5) (at 232.41 31.75 0))
    (property "Manufacturer Product Number" "AECR1206F1K10K9" (id 6) (at 232.41 31.75 0))
    (property "Descriptions" "RES 1.1k 1% 1/4W 1206" (id 7) (at 232.41 31.75 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 162.56 54.61 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP72" (id 0) (at 161.163 56.359 0))
    (property "Value" "TestPoint_Small" (id 1) (at 162.56 56.642 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 157.48 54.61 0))
    (property "Datasheet" "~" (id 3) (at 157.48 54.61 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 250.19 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q106" (id 0) (at 253.7713 96.8815 0))
    (property "Value" "PUMD3,115" (id 1) (at 253.7713 99.6566 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 250.19 97.79 0))
    (property "Datasheet" "~" (id 3) (at 250.19 97.79 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 250.19 97.79 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 250.19 97.79 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 250.19 97.79 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 250.19 97.79 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 224.79 31.75 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP77" (id 0) (at 223.393 29.689 0))
    (property "Value" "TestPoint_Small" (id 1) (at 224.79 33.782 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 219.71 31.75 0))
    (property "Datasheet" "~" (id 3) (at 219.71 31.75 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 165.1 31.75 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP73" (id 0) (at 163.703 33.499 0))
    (property "Value" "TestPoint_Small" (id 1) (at 165.1 33.782 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 160.02 31.75 0))
    (property "Datasheet" "~" (id 3) (at 160.02 31.75 0))
    (pin "1")
  )
  (symbol (lib_name "C_6") (lib_id "Device:C") (at 240.03 35.56 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C141" (id 0) (at 232.41 35.56 0))
    (property "Value" "47nF{slash}100V" (id 1) (at 227.33 39.37 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 240.9952 39.37 0))
    (property "Datasheet" "~" (id 3) (at 240.03 35.56 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB473" (id 4) (at 240.03 35.56 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 240.03 35.56 0))
    (property "Description" "CAP CER 47nF 100V X7R 0603" (id 6) (at 240.03 35.56 0))
    (property "Descriptions" "CAP CER 47nF 100V X7R 0603" (id 7) (at 240.03 35.56 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 250.19 33.02 90) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q105" (id 0) (at 250.19 26.234 90))
    (property "Value" "PUMD3,115" (id 1) (at 250.19 29.0091 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 250.19 33.02 0))
    (property "Datasheet" "~" (id 3) (at 250.19 33.02 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 250.19 33.02 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 250.19 33.02 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 250.19 33.02 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 250.19 33.02 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:D_Schottky_Filled") (at 175.26 45.72 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D6" (id 0) (at 177.8 44.7674 90))
    (property "Value" "BAS316" (id 1) (at 176.53 48.26 90))
    (property "Footprint" "Diode_SMD:D_SOD-323" (id 2) (at 175.26 45.72 0))
    (property "Datasheet" "~" (id 3) (at 175.26 45.72 0))
    (property "Descriptions" "DIODE 100V 200mA 6ns SOD323" (id 4) (at 175.26 45.72 0))
    (property "Manufacturer" "Nexperia(安世)" (id 5) (at 175.26 45.72 0))
    (property "Manufacturer Product Number" "BAS316,115" (id 6) (at 175.26 45.72 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_6") (lib_id "Device:C") (at 161.29 35.56 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C139" (id 0) (at 164.211 34.6515 0))
    (property "Value" "47nF{slash}100V" (id 1) (at 164.211 37.4266 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 162.2552 39.37 0))
    (property "Datasheet" "~" (id 3) (at 161.29 35.56 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB473" (id 4) (at 161.29 35.56 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 161.29 35.56 0))
    (property "Description" "CAP CER 47nF 100V X7R 0603" (id 6) (at 161.29 35.56 0))
    (property "Descriptions" "CAP CER 47nF 100V X7R 0603" (id 7) (at 161.29 35.56 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_name "C_6") (lib_id "Device:C") (at 241.3 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C142" (id 0) (at 233.68 78.74 0))
    (property "Value" "47nF{slash}100V" (id 1) (at 228.6 82.55 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 242.2652 82.55 0))
    (property "Datasheet" "~" (id 3) (at 241.3 78.74 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB473" (id 4) (at 241.3 78.74 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 241.3 78.74 0))
    (property "Description" "CAP CER 47nF 100V X7R 0603" (id 6) (at 241.3 78.74 0))
    (property "Descriptions" "CAP CER 47nF 100V X7R 0603" (id 7) (at 241.3 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 245.11 114.3 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP85" (id 0) (at 244.983 112.239 0))
    (property "Value" "TestPoint_Small" (id 1) (at 245.11 116.332 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 240.03 114.3 0))
    (property "Datasheet" "~" (id 3) (at 240.03 114.3 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 175.26 33.02 90) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q103" (id 0) (at 175.26 26.234 90))
    (property "Value" "PUMD3,115" (id 1) (at 175.26 29.0091 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 175.26 33.02 0))
    (property "Datasheet" "~" (id 3) (at 175.26 33.02 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 175.26 33.02 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 175.26 33.02 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 175.26 33.02 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 175.26 33.02 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 177.8 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0164" (id 0) (at 177.8 109.22 0))
    (property "Value" "GND" (id 1) (at 177.8 107.4324 0))
    (property "Footprint" "" (id 2) (at 177.8 102.87 0))
    (property "Datasheet" "" (id 3) (at 177.8 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 97.79 86.36 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 91.44 86.36 0))
    (property "Value" "GND" (id 1) (at 91.44 86.36 90))
    (property "Footprint" "" (id 2) (at 97.79 86.36 0))
    (property "Datasheet" "" (id 3) (at 97.79 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12P") (at 262.89 74.93 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0174" (id 0) (at 259.08 74.93 0))
    (property "Value" "+12P" (id 1) (at 266.0649 75.409 90))
    (property "Footprint" "" (id 2) (at 262.89 74.93 0))
    (property "Datasheet" "" (id 3) (at 262.89 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 241.6842 74.93 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP84" (id 0) (at 240.2872 72.869 0))
    (property "Value" "TestPoint_Small" (id 1) (at 241.6842 76.962 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 236.6042 74.93 0))
    (property "Datasheet" "~" (id 3) (at 236.6042 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12P") (at 189.23 73.66 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0166" (id 0) (at 185.42 73.66 0))
    (property "Value" "+12P" (id 1) (at 192.4049 74.139 90))
    (property "Footprint" "" (id 2) (at 189.23 73.66 0))
    (property "Datasheet" "" (id 3) (at 189.23 73.66 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12P") (at 186.69 31.75 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0165" (id 0) (at 182.88 31.75 0))
    (property "Value" "+12P" (id 1) (at 189.8649 32.229 90))
    (property "Footprint" "" (id 2) (at 186.69 31.75 0))
    (property "Datasheet" "" (id 3) (at 186.69 31.75 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 97.79 62.23 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR08" (id 0) (at 91.44 62.23 0))
    (property "Value" "GND" (id 1) (at 91.44 62.23 90))
    (property "Footprint" "" (id 2) (at 97.79 62.23 0))
    (property "Datasheet" "" (id 3) (at 97.79 62.23 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 152.4 73.66 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP70" (id 0) (at 151.003 71.599 0))
    (property "Value" "TestPoint_Small" (id 1) (at 152.4 75.692 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 147.32 73.66 0))
    (property "Datasheet" "~" (id 3) (at 147.32 73.66 0))
    (pin "1")
  )
  (symbol (lib_name "C_6") (lib_id "Device:C") (at 167.64 77.47 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C140" (id 0) (at 160.02 77.47 0))
    (property "Value" "47nF{slash}100V" (id 1) (at 154.94 81.28 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 168.6052 81.28 0))
    (property "Datasheet" "~" (id 3) (at 167.64 77.47 0))
    (property "Manufacturer Product Number" "AC0603KRX7R0BB473" (id 4) (at 167.64 77.47 0))
    (property "Manufacturer" "YAGEO" (id 5) (at 167.64 77.47 0))
    (property "Description" "CAP CER 47nF 100V X7R 0603" (id 6) (at 167.64 77.47 0))
    (property "Descriptions" "CAP CER 47nF 100V X7R 0603" (id 7) (at 167.64 77.47 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 177.8 74.93 90) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q104" (id 0) (at 177.8 68.144 90))
    (property "Value" "PUMD3,115" (id 1) (at 177.8 70.9191 90))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 177.8 74.93 0))
    (property "Datasheet" "~" (id 3) (at 177.8 74.93 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 177.8 74.93 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 177.8 74.93 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 177.8 74.93 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 177.8 74.93 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:TestPoint_Small") (at 149.86 31.75 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP69" (id 0) (at 148.463 28.419 0))
    (property "Value" "TestPoint_Small" (id 1) (at 149.86 33.782 0))
    (property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm" (id 2) (at 144.78 31.75 0))
    (property "Datasheet" "~" (id 3) (at 144.78 31.75 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Q_Dual_NPN_PNP_BRT_E1B1C2E2B2C1") (at 248.92 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q105" (id 0) (at 252.5013 53.7015 0))
    (property "Value" "PUMD3,115" (id 1) (at 252.5013 56.4766 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 248.92 54.61 0))
    (property "Datasheet" "~" (id 3) (at 248.92 54.61 0))
    (property "Description" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 4) (at 248.92 54.61 0))
    (property "Manufacturer" "Nexperia USA Inc." (id 5) (at 248.92 54.61 0))
    (property "Manufacturer Product Number" "PUMD3,115" (id 6) (at 248.92 54.61 0))
    (property "Descriptions" "TRANS PREBIAS NPN/PNP 6TSSOP" (id 7) (at 248.92 54.61 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
)
